**PVVNL-MT/COM/03(s)/22-23**

**PRE QUALIFYING CONDITONS & TECHNICAL SPECIFICATIONS**

1. **Turnover Requirement**: The bidder should have a minimum average annual turnover of Rs. 50.00 Lacs for best three years out of last five financial years. The audited balance sheet/CA’s certificate shall be enclosed in support of above, failing which the bid shall not be considered.
2. **GST Registration:** The Firm must be a GST registered supplier**.**

1. **SCOPE:**

This specification covers Printing & Supply of Meter Sealing Certificate Book having **Logo of PVVNL of Size 12 Cms diameter in light background printing** & is that of such a quality that once applied then should not get damaged under any circumstance viz their inspection and delivery to various Consignees of PVVNL.

Meter Sealing Certificate Book to be supplied shall have the following specification and technical features: -

4. **SHAPE AND SIZE**

(a) The Meter Sealing Certificate Book shall be of rectangular size having dimensions 32x22 Cms.

(b) The Meter Sealing Certificate Book shall contain 5x50 = 250 Sheets (50 sets of sealing certificate each set having 5 papers) in each book in different colors in following sequence:-

* 1. 1st Paper of Pink color having size 22x32 Cms & not less than 54 GSM.
  2. 2nd Paper of Yellow color having size 22x32 Cms & not less than 54 GSM.
  3. 3rd Paper of Green color having size 22x32 Cms & not less than 54 GSM.
  4. 4th Paper of Blue color having size 22x32 Cms & not less than 54 GSM.
  5. 5th Paper of White color having size 22x32 Cms & not less than 54 GSM.

1st to 4th paper shall be perforated & 5th paper shall remain intact/ fixed with Book. The paper shall be good quality i.e Sherpur/Ruchira/ABC or better.

(c) Printing on sealing certificate book shall be as per sample. Book No. and page No. shall also be printed on the sealing certificate with Serial Nos. starting from 01 to 50 for each book. The Papers used for Sealing Certificate shall be of good quality i.e not less than 54 GSM.

(d) The Meter Sealing Certificate Book shall be bound with Mill Board binding type having top cover of SBS with 230 GSM & bottom cover of Mill board of 32 ounce.

**5. SAMPLE:**

The should furnish at least 3 samples prepared by them containing all the features mentioned in Technical Specification. Tender bids not containing samples as above are likely to be rejected. The Specimen Copy is enclosed with the tender.

1. **PRICE STRUCTURE:**

The tenderers are required to quote firm prices only in every respect as per schedule available on e-procurement portal of PVVNL i.e. [**www.etender.up.nic.in**](http://www.etender.up.nic.in).

1. **SECURITY DEPOSIT:**

The Supplier shall have to deposit security @ 3% (Three Percent) of the F.O.R. destination price of the total material in the form of Bank Guarantee/Demand Draft FDR/CDR or Govt. interest bearing security duly pledged in favour of M.D., PVVNL, Meerut. The Bank Guarantee shall be in the enclosed prescribed format.

1. **SUPPLY**

The Supply shall be taken as per the approved sample.